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Abstract. As real-time systems continue to grow, performance evaluation plays a critical role in the design of these systems since the computation time, the service time, and the responsive actions must satisfy the time constraints. One of these systems is the real-time distributed multimedia-on-demand (MOD) service system. The MOD system usually fails when it misses a task deadline. The main units of the MOD system usually communicate with each other and work concurrently under timing constraints. The MOD system is designed to store, retrieve, schedule, synchronize and communicate objects comprised of mixed data types including images, text, video and audio, in real-time. In the MOD system, such data types represent the main concept of movie files. Modeling of such concurrency, communication, timing, and multimedia service (e.g. store, retrieve) is essential for evaluating the real-time MOD system. To illustrate how to model and analyze the important multimedia aspects of the MOD system, we use the Real-net (R-net) modeling technique. We choose R-net as an extension of Time Petri Net due to its ability to specify hard real-time process interaction, represent the synchronization of multimedia entities, describe concurrent multimedia activities, and illustrate the inter-process timing relationships as required for multimedia presentation. Based on modular techniques, we build three R-net performance models for describing the dynamic behavior of the MOD service system. The first model adopts the Earliest Deadline First (EDF) disk scheduling algorithm. The other models adopt the Scan-EDF algorithm. These algorithms help us to illustrate how the real-time user requests can be satisfied within the specified deadline times. Since R-nets are amenable to analysis including Markov process modeling, the interesting performance measures of the MOD service system such as the quality of service, the request response time, the disk scheduling algorithm time, and the actual retrieval time can be easily computed. In the performance analysis of the MOD models, we use our R-NET package.
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1.  Introduction

Multimedia information systems are useful in areas such as education, medicine, entertainment and space research [1, 2]. One of the most visible applications of 

multimedia information systems is the distributed multimedia-on-demand (MOD) service system. This distributed MOD system describes how to organize, store hundreds or thousands of movie files (i.e. text, images, audio, and video data) over multiple disks and allow tens of thousands of viewers (i.e. users) to concurrently access (e.g. retrieve) these movie files. The distributed MOD service system gives the user greater flexibility in choosing which movie to watch from a varied daily menu. Users can also decide when they want to see the movie they have chosen. Although these services provide flexibility, speed and a high level of efficiency, they require new support technology and considerable effort needs to be made to improve the quality of service provided by the existing systems. The storage of movies in the distributed MOD service system imposes three requirements: storage, management, and concurrent access requirements. The storage requirement is defined as the disk array architecture that needs to be occupied by hundreds or thousands of movies in digital format. The management requirement is defined as the large amount of data movie files to be managed, tens or hundreds of disks are available on-line to the user. The concurrent access requirement is defined as the large number of concurrent accesses that must be achieved to serve thousands of users at the same time.

Most recent research works have focused on the investigation of the following interesting multimedia subjects: (i) the design of several configurations to obtain an efficient and reliable multimedia storage system [3, 4], (ii) the study of various approaches that are required  to manage the traffic of real-time user requests to the storage disks [5], and (iii) the analysis of various techniques that are proposed to efficiently store and retrieve large multimedia data on/from the storage devices [1, 6-12]. These works have concentrated on constructing simulation and theoretical models for the architectures of storage part of multimedia systems to study and analyze the various problems of the available multimedia systems. Such problems are the disk load balancing problem [13], the buffer management problem [14], the reliability problem of large disk arrays [3, 4], and the problem of disk scheduling algorithms [6, 9, 10, 14-16]. Also, the augmented transition network technique [17] has been used to model the semantic aspects of a multimedia presentation, browsing, and database searching.
1.1 Related work

Petri nets (PNs) are a graphical and mathematical modeling tool applicable to many systems. As a graphical tool, it provides a natural way to represent complex logical interactions among parts or activities in information processing systems that are characterized as being concurrent, asynchronous, distributed, parallel, non-deterministic, real-time, and/or stochastic. Tokens are used in these nets to simulate the dynamic and concurrent activities of systems. As a mathematical tool, it is possible to set up state equations, algebraic equations, and other mathematical models governing the behavior of systems. PNs can be used by both practitioners and theoreticians. Thus, they provide a powerful medium of communication between them: practitioners can learn from theoreticians how to make their models more methodical, and theoreticians can learn from practitioners how to make their models realistic [18].

To provide a good means for describing temporal aspects, various timed extensions of PNs have been proposed by attaching timing constraints to transitions, places, and/or arcs. For the purpose of performance evaluation, stochastic Petri nets (SPNs) [19], generalized SPNs (GSPNs) [20], and stochastic well-formed nets [21] associate exponentially distributed firing delays to the transitions of the original PN model. These stochastic nets can be used for modeling the parallel and distributed systems.  In contrast to stochastic nets, Time Petri nets (TPNs) [22] extend the original PNs by assigning constant delays to their transitions. In [22], TPNs have been used for analyzing the recoverability of communication protocols. In [23], Timed PNs have been used to model multimedia processing synchronization scenarios. Time constraint PNs (TCPNs) [24] extend the original PNs by assigning static time intervals with constraints to transitions or places of the net. TCPNs are suitable for systems with conflict structures. 

In [25], Hierarchical Time Stream Petri nets (HTSPNs) have been used for the specification of temporal (i.e., multimedia) and logical (i.e., hypertext) synchronization within hypermedia distributed and weakly synchronous systems. In HTSPNs, the temporal non-determinism is expressed using timed arcs. In [26], Extended Object Composition PN (XOCPN) combines the logic of temporal intervals and TPNs. XOCPN is a network model and a good data structure for controlling the synchronization of multimedia presentation. XOCPN can serve as a visualization structure for users to understand the presentation sequence of media streams. XOCPN faces two problems when replaying objects in distributed multimedia systems [27]:  (1) It lacks method to describe the details of synchronization across distributed platforms. (2) It does not deal with the schedule change caused by user interactions in interactive multimedia systems. 


In [28], we have developed a new methodology to facilitate the analysis of real-time systems using Real-nets (R-nets). R-nets extend TPNs [22] by distributing probability density functions (pdfs) with uniform distributions over the time intervals associated with the transitions of the net. These pdfs are used to determine (dynamically) the state transition probability of branching from the current state to the possible next states. The structure of the R-net contains multiple tokens, multiple arcs, inhibitor arcs and two types of transitions: real-time transitions and zero-time transitions. R-net is a powerful technique for studying and analyzing the specification, verification, and temporal behavior of real-time distributed systems [28]. By R-net is a powerful technique we mean that the ability of the R-net formalism to represent classes of problems as well as the practical ability to represent a given behavior in a simpler, more compact or more natural way. Recently, the delay TPNs (DTPNs) have been developed in [29]. DTPNs extend TPNs by assigning static delay intervals to the transitions and arcs of the net. Also, it uses reduction rules to analysis the real-time systems.  The DTPN technique is close to our R-net technique. 

1.2. Contributions of this research work

This paper addresses the following important problems.

1. How to develop specification MOD models for describing the storage and retrieval processes of time-dependent multimedia data.

2. How to model the parallel (or the sequential) retrieval processes of multimedia data from multiple disks (or a single disk). 

3. How to model the real-time communication processes between the users and MOD architecture.

4. How to adopt the disk scheduling algorithms in the R-net MOD models for describing the real-time scheduling processes of the concurrent user requests.

5. How to accurately model the dynamic behavior of the MOD architecture to derive the important multimedia performance measures such as the quality of service, the request response time, the disk scheduling algorithm time, and the actual retrieval time. 

6. How to study and analyze the performance results of the R-net MOD models. Such studies can be used in designing an efficient multimedia system.

1.3. Organization of the remainder of the paper

In Section 2, we illustrate how the R-net modeling technique can be used to obtain a realistic and accurate description for real-time distributed systems. In Section 3, we describe the basic structure of the distributed MOD system.  In Section 4, we explain how the R-net technique can be used to construct Petri net models for the MOD system. We illustrate this explanation throughout two simple R-net MOD models. The first model adopts the EDF algorithm. The second model adopts the Scan-EDF algorithm. These models describe accurately the dynamic behavior of the MOD system when it receives concurrent user requests. In Section 5, we explain the construction process of building a realistic R-net MOD model. Performance measures of the R-net models of the MOD system are calculated and evaluated in Section 6. Section 7 summarizes the conclusions of our work.
2.  R-Net Modeling Technique

R-net modeling technique is one of the best suitable methodologies for studying the performance evaluation of real-time concurrent systems and distributed systems [28]. Distributing the probability density functions (pdfs) of uniform distribution over the firing intervals associated with the concurrent transitions and competitive transitions of the net can perform this study. These pdfs are used to determine (dynamically based on the overlapped intervals shown in the current state) the probabilities of branching to possible next state(s). By this way, the reachability graph obtained from the developed model can be interpreted as a Markov process.

Definition 1. A Petri net (PN) is a tuple (P,T, A, M0, W, H), where P = {p1, p2, …, pm} is a finite set of places, T={ t1, t2, …, tn} is a finite set of transitions, A ( (P(T) ( (T(P) is a finite set of arcs between places and transitions, W: A ({1, 2, 3, …} is the arc weight function, H ( (P(T),  A ∩ H = ( is an inhibition function, and M0: P(N is the initial marking function, where N is the set of natural numbers.

Definition 2.  An R-net is a tuple (PN, (, (), where 

PN: is a marked PN, called the corresponding untimed net;

(: T ( (Q+ ( 0) (Q+ ( ()  is the interval function that defines the permitted transition firing times,  where Q+  is the set of positive rational numbers, and

          (i = {[(imin, (imax] |  ( ti ( T}  with  0 ≤ (imin ≤ (imax;

(: T ( F+ is the pdf that can be distributed over the firing interval of each transition, 

     where F+   is the set of non-negative real numbers:

   F+(ti) =1              if  ti   is only an enabled (firable) transition;

   0< F+(ti) <1   if ti is an element of concurrent (parallel activities) or conflicting  (conflicting events) transitions.

From Definition 2, we should remark the following points: 

( (imin denotes the minimal time that must elapse from the time that all the input conditions of transition ti ( T are enabled. (imax denotes the maximum time that the input conditions can be enabled and the transition ti ( T must fire. Thus, in such nets, the firing of transition ti ( T takes no time, but a transition ti ( T must be enabled for a minimum time (imin and possibly up to a maximum time (imax.

( R-net adopts two types of transitions: real-time transitions (RTT) and zero-time transitions (ZTT).

Definition 3.  (Execution rule of RTT) Each ti ( RTT has a time interval [(imin, (imax]. The transition ti ( RTT is enabled as soon as its input places are marked, but firing of transition ti ( RTT could only take place within a specified time interval (. This interval is measured from the time epoch that a transition ti ( RTT is enabled. When the input conditions of transition ti ( RTT hold for a period equal to (imin ((imax), the transition ti ( RTT can (must) fire.

Definition 4. (Execution rule of ZTT) Each ti ( ZTT has a time interval [0, 0]. When the transition ti ( ZTT is enabled in a particular state, it fires immediately with probability one and cannot remain enabled for any duration of time. This concept means that the transition ti ( ZTT takes zero time to fire. Therefore, ti ( ZTT has priority over ti ( RTT. Thus, when several RTT and one ti ( ZTT are enabled in a particular state, the only a transition ti (ZTT fires with probability one.  

Definition 5. The probability density function fI((I) of a uniformly distributed random variable (I  on the time interval [(min , (max ] of a transition tI ( RTT can be formulated as follows: 

fI ((I) = 1 / [((I)max - ((I)min]  if  ((I)min ≤ (I ≤ ((I)max
Definition 6. The cumulative distribution function FI((I) of the uniformly distributed random variable (I can be formulated as follows:

Prob[((I)min ≤ (I ≤ x] = Prob((I ≤ x) = FI(x) = ∫(I   fI ((I) d(I  = (x - ((I)min) / [((I)max - ((I)min]

Theorem 1. (Firing transition probability method) When a particular state Si contains two enabled transitions (tI and tJ) and their time intervals (a ≤ (I ≤ b and c ≤ (J ≤ d) are overlapped, then either one can fire with the following probability:

Prob(tI) = ∫(I   fI ((I) [1- FJ(x)]  dx

Prob(tJ) = ∫(J   fJ ((J) [1- FI(x)]  dx 

Definition 7. (Generalized firing transition probability method) Based on Theorem 1, the general formal expression for calculating the firing probability of each fireable transition indicated in the state Si is illustrated as follows:

For I = 1 to n

Prob(tI) = [Σ 1 ≤ u ≤ k   ∫(Iu   fI (x ) (П1 ≤ v ≤ n,  v≠I   [1- Fv(x)])  dx]cond.
cond. :  If  the time interval of tI is overlapped with the time interval of tv
Then Fv(x) = [x- ((v)min ] /  [((v)max ( ((v)min ]

fI (x ) = 1 / [((I)max ( ((I)min ]

Else   Fv(x) = zero 





                                          

fI (x ) = 1 / [((I)max ( ((I)min ]

where n:  is the number of concurrent or conflicting overlapped transitions.

 k: is the number of sub-intervals in the time interval of the transition (I that overlapped with the time intervals of the other transitions. In the next section, we use some examples to illustrate the mechanism of handling the overlapped intervals.
Definition 8.  A state S of the R-net can be defined as a tuple (M, NI, RI, FS, SJ), where M is the marking function, NI is the new firing interval function, RI is the remaining firing interval function, FS is the actual firing transition function, and SJ is the sojourn time function.
Definition 9. Let us consider that the overlapped interval set (n (((min)n ≤ (n ≤ ((max)n ) shown in a state Si is associated with the enabled transition set αn. Then, the sojourn time SJ for n enabled transitions can be defined as follows: 

SJ of αn in the state Si = [((min)min of αn, ((max)min of αn]

Definition 10. Each enabled transition tI ( αn (I = 1, 2, …,n) fires from a state Si must take the following time interval (:

(min of  tI ≤  (  ≤ ((max)min of αn
Definition 11. By reaching to a state Sj from a state Si, the RIj function computes the remaining time intervals (say, (n-1) for all other transitions (say, αn-1) that still continue their firing in the state Sj, as follows:

(n-1  of  αn-1 =[ max (0,  (((min)n-1  ( (max),  (((max)n-1  ( (min)  )]

2.1. R-nets examples

In this section, we develop two R-net models to illustrate the solution steps and the verification processes of the R-net technique.

2.1.1. Example 1

In this example, we illustrate the modeling mechanism of the R-net technique as shown in Fig. 1a. Then, we illustrate the calculation processes of the Markov chain derived from the developed model under the R-net firing rules as shown in Fig. 1b. In Fig. 1, we should remark the following interesting points:

( The state configuration of the R-net sub-model of Fig. 1a is shown in Fig. 1b as follows:

S1:


S2:


S3:


S4:

M1: p1, p2

M2: p2, p3

M3: p2, p4

M4: p1, p5
NI1: 2≤(1≤5

NI2: 1≤(4≤3

NI3: 2≤(5≤5

NI4: 3≤(6≤4

      : 3≤(2≤6 

      : 4≤(3≤8

RI1: 0


RI2: 0≤(3≤6

RI3: 0≤(3≤5

RI4: 0≤(1≤1










      : 0≤(2≤2

FS1: (t1, ( t2) // t3
FS2: t3 // t4

FS3: t3 // t5

FS4: t1, ( t2 

SJ1: [2,5]

SJ2: [0,3]

SJ3: [0,5]

SJ4: [0,1]
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(b) Markov processes of the R-net model

From M, to Ms: Prob[t;]= (d+c-2a)/ 2(b-a) = 0.33 From M, to Mg: Prob[ts]= (2b -d-c)/ 2(b-a) = 0.67
From M, to My: Prob[t,]= (b-a)/ 2(d-c) = 0.25 From My to M,: Prob[t;|= (2d-b-a)/ 2(d-a) = 0.75
From M; to My: Prob[ts]= (2bd-2ad+2ac-b*-c?) / 2(b-a)(d-c) = 0.7

From M; to Mg: Prob[ts]= (b-c)*/ 2(b-a)(d-¢) = 0.3

(c) Calculation of the transition state probabilities of the markov processes shown in Fig. (b)




Fig. 1. An illustration of solution steps of the R-net modeling technique.
( In the function FSi, the mark // denotes concurrency behavior and the mark ( denotes conflicting behavior.

( In Fig. 1b, the transition probabilities from a state S1 to states S2, S3 and S4 are calculated based on both Theorem-1 and the overlapped intervals associated with a state S1 as follows:

Prob(t1) = Σ 1 ≤ u ≤ 3    ∫(1u  f1 (x)  (П1 ≤ v ≤ 3,  v≠I    [1-Fv(x)]) dx 

= ∫(11 f1 (x) dx + ∫(12 f1 (x) [1-F2(x)] dx + ∫(13  f1 (x) [1-F2(x)] [1-F3(x)] dx

 where a ≤ (11 ≤ c,  c ≤ (12 ≤ e,  e ≤ (13 ≤ b

Prob(t2) = Σ 1 ≤ u ≤ 2    ∫(2u  f2(x)  (П1 ≤ v ≤ 3,  v≠I    [1-Fv(x)]) dx 

= ∫(21 f2 (x) [1-F1(x)] dx + ∫(22 f2 (x) [1-F1(x)] [1-F3(x)] dx

 where c ≤ (21 ≤ e,  e ≤ (22 ≤ b  

Prob(t3) = Σ 1 ≤ u ≤ 1    ∫(3u  f3(x)  (П1 ≤ v ≤ 3,  v≠I    [1-Fv(x)]) dx 

= ∫(31 f3 (x) [1-F1(x)] [1-F2(x)] dx

 where e ≤ (31 ≤ b 

In these equations, we should remark the following: 

  f1(t) = 1  ( (b - a), 
   F1(t) = (t - a)  ( (b - a),           f2(t) =1  ( (d - c), 

  F2(t) = (t - c)  ( (d - c),        f3(t) = 1  ( (f - e), and            F3(t) = (t - e)  ( (f - e).

( In Fig. 1c, we illustrate the calculation of the transition probabilities of the other states that are shown in Fig. 1b.
2.1.2. Example 2

In Fig. 2a, we describe a complete R-net model with its time intervals. The structure of this model incorporates the parallel, sequential, conflict, and synchronous events that can occur in the real-time computer systems. The R-net technique is able to model such events as follows. Transitions t1 and t2 model the conflict (decision, choice) event. Transitions t3 and t4 model the concurrent (parallel) event. Transition t5 models the synchronization event. In Fig. 2b, we describe the complete Markov chain of the model shown in Fig. 2a. This description is like that of Figs. 1b and 1c. To verify from the correctness of the developed R-net model, the following conditions must be satisfied in its Markov processes:
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Fig. 2. An illustration of solution steps and verification processes of the R-net model shown in Fig. 2a.
1. An R-net model is said to be k-bounded if the number of tokens in each place does not exceed a finite number k for any marking Mi reachable from the initial marking M0.

2. An R-net model is said to be live (guarantees deadlock-free operation) if every transition in the model is fire.

3. An R-net model is said to be reversible if, for each marking Mi in the Markov process of this model, M0 is reachable from Mi. Thus, in a reversible net one can always get back to the initial state M0.

4. An R-net model is said to be persistent if, for any two enabled transitions (ti, tj) the firing of one transition (ti) will not disable the other (tj). A transition in a persistent net, once it is enabled, will stay enabled until it fires. Persistency is closely related to conflict-free nets.

In Fig. 2b, all these conditions are satisfied. It is interesting to note that the solving steps, firing rules, and verification processes of the R-net technique have been automated through our R-NET package [28].

2.2. Solution technique for R-nets
Since the R-net comprises the ZTT and RTT transitions, the states of this net can be classified into the flash and exact states, respectively. The behavior of the reachability set of R-net model is recognized as Embedded Markov Chain (EMC) [28]. Thus, the EMC comprises both flash and exact states. Each flash state (i.e. time interval [0, 0]) in the EMC can be eliminated (because it represents the logical behavior of the modeled system) as follows. Since the probability of firing the transition ti ( ZTT from the flash state is one, the state-transition probability from the flash state to its next state is also one. Thus, we can simply remove the flash state by directly connecting its preceding state to its next state. After removing the flash state from the EMC, we call it a reduced EMC (REMC). A REMC comprises only “exact” states.

The stationary embedded probabilities X(S) of the REMC can be obtained from the state-transition probabilities Q(Si, Sj) by solving a system of simultaneous linear equations.



(1( j (N  Q(Si, Sj)  X(Sj) = X(Si), 

i = 1,2,…,N  

(1( i (N  X(Si) = 1





          

 (1)

where N denotes the number of “exact” states in the REMC. Let ASJi be the average sojourn time in a state Si for αn transitions. ASJi can be calculated as follows: 



ASJi = ([((min)min + ((max)min] of αn) ( 2                                   
  
 (2)

The steady state probabilities of the REMC ((1, (2, …, (N) are calculated as follows:



(i = ((Si) = (X(Si) ( ASJ(Si)) (  (1( j (N X(SJ)


   
(3)

From these steady probabilities, one can compute several generic performance measures [28]. The calculation processes of the steady state probabilities of the derived Markov chain from the developed R-net model have been automated through our R-NET package [28]. 

3.  Mod Architecture

Several architectures and configurations for efficient storage, reliable storage, and delivery of multimedia data have been proposed and utilized such as MPEG-1, MPEG-2, MPEG-4, H.261, Berkeley, INDEO, Oracle media system, Microsoft tiger multimedia file system, Hong Kong telecom interactive multimedia service system [1,2,5, 8-10, 14, 30]. The main objective of our work is to develop a modeling technique has the capability of modeling, analyzing, and studying such architectures in an easy way. Therefore, we have adopted the basic multimedia aspects of such architectures in the distributed MOD service system shown in Fig. 3. The distributed MOD system consists of: (i) a central multimedia server, (ii) a wide area network, (iii) a group of Local Multimedia Servers (LMS: LMS1, LMS2,…, LMSn), and (v) a group of User Display Equipment (UDE: UDE1, UDE2, …, UDEm). Each LMSi (LMS is connected through an ATM interconnection network to its own group of UDE. Thus, the MOD system illustrates the main features of the available multimedia systems [2, 8, 10, 12, 30]. A brief description of the MOD components is given below.

3.1. User display equipment (UDE)

The UDE is a group of intelligent display units. Each UDEj (UDE can be represented as a computer has the capability of sending / receiving multimedia user request(s) to/from the LMSi (LMS. 

3.2. Central multimedia server (CMS)

The CMS consists of a main server, a network controller, and hundreds of gigabyte disks. These disks are used as an archive containing all the original movie files that can be requested by the users. The CMS uses a high-speed network (e.g. ATM switching technology [5, 12, 30]) to send copies of these movie files to each LMSi (LMS. 

3.3. Local multimedia servers (LMSs)

Each LMSi (LMS is a system which comprises a main server, a network controller, a high-speed network, a group of disk servers (DS: DS1, DS2, …, DSn), a group of buffers (BF: BF1, BF2, …, BFn), and a group of storage disk arrays [6, 8, 10-13]. Each storage disk array (SDA: SD1, SD2, …, SDk) has the capability of storing a subset of the total set of movie files. Each disk server DSx ( DS has a local storage disk SDk ( SDA and a local buffer BFi(BF. The network controller of LMSi ( LMS is responsible for receiving the incoming multimedia user requests from the UDEj ( UDE and sending them to its main server. The main server has the capability of controlling and accessing any disk server DSx ( DS through a high-speed network. By this way, the various storage disks of LMS are managed separately, from both the logical and physical point of view.  

3.3.1. Storing process of the movie files

The transfer of movie files from the CMS to each disk array in the LMSi ( LMS is performed based on off-line approach [31] as follows. The network controller of each LMSi ( LMS receives some of popular movie files from the CMS. The network controller, then, forwards these movie files to its main server. The main server splits and distributes the received popular movie files among all storage disks in its disk array. In each LMSi (LMS, the main server splits each data file to be stored into macro blocks of a pre-established size, called streams. In turn, streams are split into blocks called segments, which are distributed over the various storage disks of LMSi ( LMS. By this way, the main server has the capability of reading these segments concurrently from each storage disk SDk ( SDA in the disk array of LMSi (LMS. This parallel retrievability aspect represents the important advantage of storing each movie file as segments over the disk array. According to this storing aspect, the main server of LMSi ( LMS serves the user request by retrieving the segments of the desired movie file and reassembling the data segments into contiguous blocks or streams to satisfy the multimedia request.

3.3.2. Serving process of the user request

To know the allocation places of storing the segments of each movie file over the various storage disks of the desired array, the main server of each LMSi ( LMS constructs an allocation map for each stored movie file into its disk array. Once the main server of LMSi ( LMS receives the multimedia requests from its network controller, it starts to serve these requests as follows. It downloads the desired allocation map of each target movie file to all its disk servers. Then, the main server uses the allocation map to schedule the deadline times of the requested movie files (TRM). Subsequently, the main server executes the accepted user requests. This schedule process can be done by using one of the available disk scheduling algorithms [9, 11, 14-16]. For example, the Earliest Deadline First (EDF) algorithm and the Scan-EDF algorithm. Such algorithms avoid starvation of service to requests. In fact, the main aim of disk scheduling algorithms is to manage multimedia traffic and allow performance improvements (i.e. maximize throughput) by meeting all the deadline times of the user requests.

    The following equation illustrates the different parameters that effect on the deadline times of the requested movie file j (TRMj): 

                                      TRMj = TRS + TSB + TAS + TSS



  (4)

where

TRMj: is the deadline time of the requested movie file j. The user has to receive his requested movie file j before the TRMj time.

TRS: is the deadline time of retrieving the desired segments. It denotes the times estimated by the disk servers (DS) of LMSi ( LMS to retrieve all the segments of the desired movie file from their disk array (SDA). By using parallel retrieving approach, TRS = max {TRS1, TRS2, …, TRSn}. The parameter n represents the number of the desired segments. From this equation, the disk server DSj ( DS of LMSi ( LMS spends TRSn ( TRS time to retrieve a segment-n from its storage disk SDk ( SDA.

TSB: is the deadline time of storing the desired segments into buffers. It denotes the time estimated by the disk servers (DS) of LMSi ( LMS to store the retrieved n-segments of the desired movie file into their local buffers. By using parallel storing approach, TSB = max {TSB1, TSB2, …, TSBn}. The parameter n represents the number of the desired segments. From this equation, the disk server DSj ( DS of LMSi (LMS spends TSBn ( TSB time to store a retrieved segment-n into its local buffer. 

TAS: is the deadline time of reassembling the desired segments. It denotes the time estimated by the main server of LMSi ( LMS to reassemble all the retrieved segments of the desired user request into composed streams. By using parallel reassembling (RSS) approach, TAS = max {RSS-stream-1, RSS-stream-2, …, RSS-stream-m}. The parameter m represents the number of the desired streams. These streams are constituted from the composed segments of the requested movie file.  

TSS: is the deadline time of sending the desired streams. It denotes the time estimated by the main server of LMSi ( LMS to send all streams to the requested user through its network controller. Sending processes of streams can be done by using pipeline approach as follows: TSS=max {send-stream-1, send-stream-2, …, send-stream-m}.

As a conclusion, each LMSi ( LMS starts to serve the user request by collecting the desired segments of the requested movie file. Then, it reassembles these streams. Finally, it sends these streams to the requested user within the TRMj time.

4.  R-net Model for a Simple Mod Architecture

To illustrate the dynamic behavior of the MOD system shown in Fig. 3, we have used the R-net modeling technique. The R-net technique has the capability of describing the interaction between the real-time processes that are required for multimedia presentation. By incorporating such R-net aspects into the developed model, we can easily build an R-net multimedia model has with ability to capture the time dependencies of multimedia data presentation, indicate the sequential and parallel multimedia activities, and describe how to store, retrieve, schedule, and communicate multimedia data. To illustrate the mechanism of constructing an R-net model for the complicated MOD architecture shown in Fig. 3, we have developed two models. The first R-net model describes the dynamic behavior of the MOD architecture in a simple way. The second R-net model describes the dynamic behavior of an exact MOD architecture. In this section, we discuss the simple R-net MOD model. In the next section, we discuss the exact R-net MOD model.

           Based on the following concept, we have developed a simple R-net model for the MOD architecture shown in Fig. 3. In this model, a user UDEj ( UDE sends a multimedia request to the main server of LMSi ( LMS. This LMSi ( LMS has three disk servers DSx, DSy, and DSz ( DS with their storage disks SDk1, SDk2, and SDk3 ( SD and their local buffers BF1, BF2, and BF3 ( BF, respectively. The requested movie file has been stored in the storage disks SDk1, SDk2, and SDk3 ( SD, as explained in Section 3. 3. 1. The disk server DSx ( DS handles the main part of the requested movie file. The disk server DSx ( DS sends control signals to the disk servers DSy ( DS and DSz ( DS to retrieve the remaining parts of the requested movie file. For better understanding, we have used the modular approach to develop such R-net model. Thus, the developed R-net MOD model consists of the following sub-models. 
4.1. Sub-model of the receiving mechanism of the main server

The R-net model shown in Fig. 4 describes how the following processes can be implemented. The main server of LMSi ( LMS receives the user request through the ATM switching network. The main server of LMSi ( LMS uses its map allocation to determine the disk servers and their storage disks that contain the required segments of the requested movie file. The main server communicates with its disk servers DSx, DSy, and DSz ( DS. The disk servers DSx, DSy, and DSz ( DS communicate with their storage disks SDk1, SDk2, and SDk3 ( SD, respectively. Based on these communication processes, the main server performs a comparison process on the queue status of the disk servers SDk1, SDk2, and SDk3 ( SD. As a comparison result, the main server selects the disk server and its storage disk that has a fewer queues to handle the user requests.
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Fig. 3.  MOD architecture.
[image: image4.png]p1: A user submission.

P2 An UDE_] <UDE.

t1. A user uses his UDE; ¢ UDE to prepare his requested movie file.

ps: A network controller of UDE; € UDE receives the user request.

ps: An ATM switching network.

ta: A network controller of UDE; eUDE transmits a user request to the desired
LMS; eLMS through the ATM switching network.

ps: A user request is passing through the ATM switching network.

ps: A network controller of LMS; e LMS.

pr: An LMS; € LMS is idle.

t3: A network controller receives the user request.

ps: A network controller is ready to send the user request to its main server.

po: The main server is idle.

ty: The main server receives the user request.

pio: The map allocation of the requested movie file.

pu: The main server downloads the map allocation of the requested movie file.
The main server uses this map to determine the group of storage disks that
contain the required segments of the requested movie file.

ts: The main server sends control signals to the disk servers (DS: DSy, DS,, and
DS.) of the desired storage disks (SD: SDii, SDi,, and SDis). Then, each
disk server checks the queue status of its attached storage disk.

piz: The main server interrogation being received by DS, €DS.

pis: The main server interrogation being received by DS, eDS.

pis: The main server interrogation being received by DS, €DS.

te: A disk server DS, €DS sends a reply signal to its main server.

tz: A disk server DS, DS sends a reply signal to its main server.

ts: A disk server DS, €DS sends a reply signal to its main server.

pi: The main server receives a reply signal from DSy €DS.

pis: The main server receives a reply signal from DS, eDS.

pi7: The main server receives a reply signal from DS, €DS.

to: The main server performs a comparison process on the queue status of the
disk servers DSy, DS,, and DS,.

pis: A comparison result. Based on this comparison result, the main server
decides which disk server has a fewer queues. The selected disk server will
be used to handle the user request (s).

tio: The main server selects a disk server DS, €DS to handle the desired user
request(s). To allow the proposed model to handle more than one user
request, the main server of LMS; eLMS will proceed to an idle state (after
tio fires) to become ready to handle another user request.

pis: The state of queued requests.





Fig. 4. R-net model of the main server of LMSi (LMS.

4.2. Sub-model of executing the EDF scheduling algorithm by the disk server      DSx ( DS

From the user requests waiting to be served, the EDF algorithm selects the one with the earliest deadline time and serves it. If various requests have the same deadline time, they are served on FIFO policy. As pointed out, the main server of LMSi ( LMS receives the accepted user requests from its network controller. Then, the main server divides each user request into multiple segments (i.e. n-segments) and sends the segment requests (SR: SR1, SR2,…, SRn) with their deadline times (TRS: TRS1, TRS2, …, TRSn) to all its disk servers (DS: DS1, DS2, …, DSm) concurrently. Subsequently, each disk server DSx ( DS accesses its storage disk to retrieve the requested segment(s). To understand the schedule policy of the EDF algorithm, we use the following example.

Example.  Let us assume that there is a queue of unsorted segment requests at the disk server DSx ( DS of LMSi ( LMS.  Such requests are SR1, SR2, SR3, SR4, and SR5 with their deadline times TRS: TRS1 = 700, TRS2 = 800, TRS3 = 600, TRS4 = 500, and TRS5 = 500, respectively. The disk server DSx ( DS uses the EDF algorithm to perform the following steps before serving any of them.

Step 1. The disk server DSx ( DS starts to arrange the unsorted segment requests in ascending order according to their deadline times. In this example, the DSx (DS uses the EDF policy to schedule the segment requests as follows: SR4, SR5, SR3, SR1, and SR2.

Step 2. If some of segment requests have equal deadline times, then the EDF algorithm uses the FIFO technique to select the one to be served before the others. In this example, the EDF uses the FIFO technique to handle the segment requests SR4 and SR5.

 Step 3. The disk server DSx ( DS serves the segment requests according to their arrangement. In this example, the DSx ( DS uses the EDF technique to serve the segment requests SR3, SR1, and SR2.

The R-net model shown in Fig. 5 describes the dynamic behavior of the disk server DSx ( DS when it applies the steps of the EDF algorithm on the unsorted segment requests.

4.3. Sub-model of executing the Scan-EDF scheduling algorithm by the disk server DSx ( DS

This algorithm represents a scan type of disk scheduling algorithm. In the Scan-EDF algorithm, each disk server DSx ( DS of LMSi ( LMS can handle its queue segment requests as follows:

If  
the segment requests do not have the same segment deadline times,

Then 
the segment requests can be served according to the EDF scheduling algorithm,

Else  
the segment requests can be served according to their track locations on the disk. This service can be done by modifying the deadline time of retrieving segments (TRS) through the following equation:

MTRSj = TRSj + (Nj / Nmax –1) 




   
(5)

where

TRSj:    Deadline time of retrieving a segment request SRj,

Nj :       Track position of the data of a segment request SRj,

Nmax :     Maximum track number on the disk,

MTRSj : Modified deadline time of retrieving a segment request SRj.
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Fig. 5. R-net model of the EDF disk scheduling algorithm.

Example.  Suppose the segment requests SR1, SR2, SR3, and SR4 have deadline times TRS: TRS1 = 500, TRS2 = 500, TRS3 = 500, and TRS4 = 600, respectively. They ask for data from tracks 347, 113, 851, and 256, respectively. Based on equation 5, if Nmax = 1000, the modified deadline times of SR1, SR2, SR3, and SR4, become MTRS1 = 499.347, MTRS2 = 499.113, MTRS3 = 499.851, and MTRS4 = 599.256, respectively. When these requests are served by their modified deadline times, segment requests SR1, SR2, and SR3, are served in the Scan order of SR2, SR1 and SR3; SR4 is served later. 

The R-net model shown in Fig. 6 describes the dynamic behavior of the disk server DSx (DS when it performs the steps of the Scan-EDF algorithm on the unsorted segment requests.
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Fig. 6. R-net model representing Scan-EDF scheduling algorithm.

4.4.  Sub-model of the retrieving mechanism of the disk server DSx ( DS

The R-net model shown in Fig. 7 illustrates the sequential and parallel retrieving processes of the requested movie files from the disk array architecture. Also, it illustrates how the retrieving operation of the requested movie file can be performed within the specified deadline time. In fact, this model describes how the following processes can be implemented. Let us assume the LMSi ( LMS has three disk servers DSx, DSy, and DSz ( DS with their storage disks SDk1, SDk2, and SDk3 ( SD and their local buffers BF1, BF2, and BF3 ( BF, respectively. The disk server DSx ( DS has a fewer queues into its storage disk SDk1.  Thus, the main server chooses the disk server DSx ( DS to handle the user request. Then, the main server allows the disk server DSx ( DS to retrieve the segments of the requested movie file from its storage disk SDk1 ( SD and store the retrieved segments into its local buffer BF1 ( BF. In parallel, the disk server DSx ( DS sends control signals to disk servers DSy, and DSz ( DS to retrieve the remaining parts of the desired segments from their storage disks SDk2, and SDk3 ( SD and to store them into their buffers BF2, and BF3 ( BF. Then, the disk server DSx ( DS collects and stores all the desired segments into its buffer BF1 ( BF. Finally, the main server composes the segments of the requested movie file into streams.

4.5. Sub-model of the sending mechanism of the main server of LMSi  ( LMS

The R-net model shown in Fig. 8 describes how the following processes can be implemented. The main server sends the composed streams to the requested UDEj ( UDE through the ATM switching network. The UDEj ( UDE sends +ACK message or –ACK message to the main server of LMSi ( LMS. The requested user UDEj ( UDE receives and displays the composed streams of the requested movie file.

From the above-mentioned sub-models, it is interesting to note the following. Figs. 4, 5, 7, and 8 describe the R-net MOD model when it executes the EDF disk scheduling algorithm. Figs. 4, 6, 7, and 8 describe the R-net MOD model when it executes the Scan-EDF disk scheduling algorithm.

5.   R-net Model for an Exact Mod Architecture

The R-net MOD model shown in Figs. 4, 5 (or 6), 7, and 8 illustrates the different multimedia processes that can occur when a user UDEj ( UDE accesses a disk server DSx ( DS of LMSi ( LMS. We have developed this model in a simple and an easy way by using a modular technique to facilitate understanding how the exact R-net MOD model can be constructed. Thus, the R-net MOD model shown in Fig. 9 illustrates the retrieving, scheduling, synchronization, sequential, concurrent, and communication multimedia processes that can occur between multiple users and multiple LMSs. In each LMSi ( LMS, there are three disk servers DSx, DSy, and DSz ( DS work concurrently to satisfy the requested movie files. In other words, these disk servers can work concurrently to retrieve the segments of three requested movie file at the same time. Based on a modular technique, we have constructed the R-net MOD model shown in Fig. 9. Throughout four sub-models incorporated in this model, we describe the following interesting multimedia processes that can occur when multiple users access the distributed MOD system of Fig. 3.
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Fig. 7. R-net model for describing retrieving processes of the desired segments of the requested movie file from the disk servers of LMSi ( LMS: DSx, DSy, and DSz ( DS.
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Fig. 8. R-net model for describing the communication processes between LMSi ( LMS and UDEj ( UDE.

Sub-model-I describes the transmission processes of the requested movie files from multiple users to multiple LMSs through the ATM switching network. This sub-model starts from p1 and t1 to t9 and p18. The meanings of places and transitions of this sub-model are the same as those of Fig. 4. In this sub-model, we use the token properties of the Petri net technique to represent the access processes of multiple users to the MOD system. This description can be done by changing: (i) the number of tokens shown in place p1 to become proportional with the number of users, and (ii) the number of tokens shown in place p7 to become proportional with the number of LMSs.


Sub-model-II describes the sequential and parallel operations of disk servers DSx, DSy, and DSz ( DS when they execute the Scan-EDF disk scheduling algorithm on the user requests. The following parts describe the dynamic behavior of this model:

( Part-IIA describes the dynamic behavior of the disk server DSx ( DS when it executes the Scan-EDF algorithm. This part starts from p19 to p25. The meanings of the places and transitions of DSx ( DS model are the same as those of Fig. 6.

( Part-IIB describes the dynamic behavior of the disk server DSy ( DS when it executes the Scan-EDF algorithm. This part starts from p33 to p39. The meanings of the places and transitions of the DSy ( DS model are the same as those of Fig. 6.

( Part-IIC describes the dynamic behavior of the disk server DSz ( DS when it executes the Scan-EDF algorithm. This part starts from p47 to p53. The meanings of the places and transitions of DSz ( DS model are the same as those of Fig. 6.


Sub-model-III describes the dynamic behavior of the disk servers DSx, DSy, and DSz ( DS when they retrieve the required segments from the storage disks SDk1, SDk2, and SDk3 ( SD, respectively. Also, it illustrates the sequential and parallel processes of these disks when they communicate with each other. The following parts describe the dynamic behavior of this sub-model:  

( Part-IIIA describes the dynamic behavior of the disk server DSx ( DS when it retrieves the main part of the requested segments from its storage disk SDk1 ( SD and sends control signals to the disk servers DSy, and DSz ( DS to retrieve the remaining parts of the requested segments from their storage disks SDk2, and SDk3 ( SD, respectively. The model of the disk server DSx ( DS starts from p26 to p32. The meanings of the places and transitions of the DSx ( DS sub-model are the same as those of Fig. 7.

( Part-IIIB describes the dynamic behavior of the disk server DSy ( DS when it retrieves the main part of the requested segments from its storage disk SDk2 ( SD and sends control signals to the disk servers DSx, and DSz ( DS to retrieve the remaining parts of the requested segments from their storage disks SDk1, and SDk3 ( SD, respectively. The model of the disk server DSx ( DS starts from p40 to p46. The meanings of the places and transitions of the DSy ( DS sub-model are the same as those of Fig. 7.

( Part-IIIC describes the dynamic behavior of the disk server DSz ( DS when it retrieves the main part of the requested segments from its storage disk SDk3 ( SD and sends control signals to the disk servers DSx, and DSy ( DS to retrieve the remaining parts of the requested segments from their storage disks SDk1, and SDk2 ( SD, respectively. The model of the disk server DSx ( DS starts from p54 to p60. The meanings of the places and transitions of the DSz ( DS sub-model are the same as those of Fig. 7.

Sub-model-V describes the transmission processes of the composed streams of the requested movie file from the main server of LMSi ( LMS to the requested UDEj ( UDE through the ATM switching network. The meanings of the places and transitions of this sub-model are the same as those of Fig. 8.

6.  Performance Evaluation

In this section, we study and analyze the important performance measures that can be calculated from the following R-net MOD models: 

( From the sub-models shown in Figs. 4, 5, 7, and 8, we construct a simple R-net MOD model adopts the EDF disk scheduling algorithm. We call it a model-A.

( From the sub-models shown in Figs. 4, 6, 7, and 8, we construct a simple R-net MOD model adopts the Scan-EDF disk scheduling algorithm. We call it a model-B.

( The R-net MOD model shown in Fig. 9 is called a model-C. This model adopts the Scan-EDF disk scheduling algorithm.

Based on the solution steps of the R-net technique (explained in Section 2) and the solving processes of our R-NET package [28], the required performance measures can be calculated. To obtain realistic performance results, we have associated the R-net transitions with real-times obtained from the benchmark data sets of actual multimedia systems [2, 6, 7, 16, 30]. To save space, we have omitted these times.

6.1. Performance measures

I. Quality of service (QoS)

The QoS is the most important performance measure for the multimedia systems [14, 15]. The QoS can be defined through the following aspects:

( The interruption probability: the probability that the requested movie file is not available. To incorporate such aspect in the developed R-net MOD models, we have added a transition tinterruption to the first R-net sub-models shown in Figs. 4, and 9. Fig. 10 illustrates this modification. 

( The data loss probability: the probability of occurrence the buffer overflow problem. In our models, we assume that each disk server in the LMSi (LMS has a finite buffer size. Thus, it is possible to overflow any buffer. To incorporate such aspect in the developed R-net MOD models, we have modified the disk server sub-models shown in Figs. 7 and 9 as shown in Figs. 11   and 12, respectively. The disk server DSx (DS sub-model shown in Fig. 7 is modified in Fig. 11. In this modification, we add a transition toverflow to a place p32 and inhibitor arc to a transition t18 from a place p27. Similarly, the sub-models of the disk servers DSx,  DSy, and DSz  (DS shown in Fig. 9 are modified in Fig. 12. 
According to the R-net technique (explained in Section 2), the interruption probability (or the data loss probability) associated with the transition tinterruption (or the transition toverflow) is determined dynamically in each state this transition has the ability to fire. For more detail, see examples 1 and 2. In fact, such dynamically behavior is the main advantage of using the R-net technique.

( The request response time (RRT): the user has to receive his requested movie file before the deadline time of this request. The concept of the RRT is explained mathematically through the TRMj time shown in Eq. 4. We have already incorporated this concept in the developed R-net MOD models, as explained in Sections 4 and 5. Also, we have attached the required deadline times with the transitions of these models.

By incorporating the interruption probability and the data loss probability in the R-net MOD models, we can easily calculate the RRT and QoS performance measures in accurate way. To calculate the RRT performance measure, we run the R-net model. Then, we derive the Markov processes and calculate the steady state probabilities of this model. Finally, the RRT can be calculated as follows:

RRT = ASJ1 / (1 




                
 (6)

where 

ASJ1   is the average sojourn time of the initial state S1;

(1       is the steady state probability of the initial state S1;

S1    is the initial state of model-A, model-B, or model-C when a place p1 contains one (or more) token(s).


The Quality of Service the MOD system provides can be evaluated according to the following expression:

QoS = Nmr  (  (RRT ( NDs)



               
(7)

where

RRT   is the response time of the multimedia requests.

Nmr    is the number of multimedia requests.

NDs    is the number of disk servers in the LMSi (LMS.
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Fig. 9.  An exact R-net MOD  model.


	p1 : A user submission

p11: The main server of LMSi ( LMS downloads the map allocation of the requested movie file. This map contains the available movie files. The main server uses this map to determine the group of storage disks that contain the required segments of the requested movie file. As pointed out, these storage disks are SDk1, SDk2, and SDk3 and their disk servers are DSx, DSy, and DSz, respectively

t5: The main server checks the status of queues at the storage disks SDk1, SDk2, and SDk3 through their disk servers DSx, DSy, and DSz, respectively.

tinterruption: The main server sends an interruption signal to the requested user. This signal means that the requested movie file is not available. Aftertime, the user can send his request.


Fig. 10.  A modification for the R-net MOD models (model-A, model-B, and model-C) to handle the interruption problem.
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Fig. 11. A modification for the disk server DSx ( DS submodel shown in Fig. 7 to handle the buffer overflow problem.
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Fig. 12. A modification for the submodels DSy ( DS ,  DSy ( DS and DSz ( DS shown in Fig. 9  to handle the buffer overflow problem.

II. Disk scheduling algorithm time (DSAT)

DSAT is defined as the time taken by the EDF algorithm or the Scan-EDF algorithm to schedule the user requests. From the calculation of DSAT, we can easily study the efficiency of the distributed MOD system under the different types of disk scheduling algorithms.

● To study the R-net EDF sub-model shown in Fig. 5, the output of place p29 must be connected to a transition tconnect (new transition added to the sub-model) and the output of transition tconnect to a place p19. Putting one (or more) token(s) in the place p19 derives the Markov process of this sub-model. After deriving the Markov processes and obtaining the steady state probabilities, the DSAT can be calculated as follows:

DSAT of EDF algorithm = ASJ19 / (19  




  (8)

where

ASJ19    is the average sojourn time of the state S19;

(19         is the steady state probability of the state S19;

S19         is the initial state of the R-net EDF sub-model when p19 contains one token.

● To study the R-net Scan-EDF sub-model shown in Fig. 6, the output of place p26 must be connected to a transition tconnect (new transition added to the sub-model) and the output of transition tconnect to a place p19. Based on Eq. 8, the DSAT of Scan-EDF can be calculated.

 ● To study the R-net Scan-EDF sub-model shown in Fig. 9, we remove it from the complete model. Then, the output of places p26, p40, and p54 must be connected to a transition tconnect and the output of transition tconnect to a place p18. Based on Eq. 8, the DSAT of this model can be calculated.

III. Actual retrieval time (ART)

ART is defined as the time taken by the main server of LMSi ( LMS to collect the data of the desired movie file from the storage disk array of LMSi ( LMS. 

( To study the R-net retrieval sub-model shown in Fig. 7, the output of transition t23 must be connected to a place p26. After deriving the Markov processes and obtaining the steady state probabilities, the ART can be calculated as follows:

ART = ASJ26 / (26  
                                                  
(9)

where

 ASJ26     is the average sojourn time of the state S73.

 (26       is the steady state probability of the state S73.

 S26     is the initial state of the R-net retrieval sub-model when a place p26 contains one (or more) token(s).

( To study the R-net retrieval sub-model shown in the complete R-net model of Fig. 9, we remove it from this model. Then, the output of transitions t23, t37, and t51 must be connected to a place pconnect and the output of this place to a transition tconnect. The output of tconnect must be connected to the places p26, p40, and p54. In this case, the initial token(s) of this sub-model starts from a place pconnect. After deriving the Markov processes and obtaining the steady state probabilities, the ART can be calculated as follows:

ART = ASJconnect / ( connect  




(10)

where

 ASJ connect     is the average sojourn time of the state S connect.

 (connect        is the steady state probability of the state S connect.

 S connect     is the initial state of the R-net retrieval sub-model when place pconnect contains one (or more) token(s).

6.2. Performance analysis

By using the R-NET package [28], the results of the performance measures such as Quality of Service (QoS), Request Response Time (RRT), Disk Scheduling Algorithm Time (DSAT), and Actual Retrieval Time (ART) can be calculated. In the following, we study and analyze the results of these performance measures. 


Table 1 illustrates the DSAT performance results obtained from the EDF sub-model shown in Fig. 5 and the Scan-EDF sub-model shown in Fig. 6. From these results, we observe that the Scan-EDF algorithm gives 17% - 23% improvement compared to the EDF algorithm. Thus, we can conclude that the Scan-EDF algorithm performs better than the EDF algorithm. This conclusion is agreed with that obtained by a simulation method shown in [16]. Furthermore, the simulation results of the disk scheduling algorithms presented in [16] have been obtained in a few hundred milliseconds like our performance results. For example, in [16], the simulation result of the Scan-EDF algorithm for 6 multimedia requests is approximately 800 msec. Thus, the proposed modeling technique introduces an easy way to verify from the dynamic behavior and the execution time of a new disk scheduling algorithm.  

Table 1.  The results of the DSAT performance measure (msec)

	Nmr
	EDF sub-model

(shown in Figure 4)

(sub-model-II in model-A)
	Scan-EDF sub-model

(shown in Figure 5)

(sub-model-II in model-B)

	1
	180.608
	137.908

	2
	329.395
	266.397

	3
	478.584
	394.509

	4
	628.456
	519.481

	5
	775.064
	641.564

	6
	914.192
	767.918



Table 2 illustrates that the ART performance results obtained from the retrieval sub-model shown in Fig. 9 are better than those of Fig. 7 due to the following reason. The simple retrieval sub-model shown in Fig. 7 describes the dynamic behavior of the disk server DSx (DS when it retrieves the requested movie file. Such disk server performs the retrieval processes of the requested movie files in a sequential manner. In contrast, the realistic retrieval sub-model shown in Fig. 9 describes the dynamic behavior of the three disk servers DSx, DSy, and DSz (DS when they work together in a parallel manner to retrieve the requested movie files. The effect of these parallel retrieval processes especially appears when the number of requests is three. 


Table 2 also confirms that when both sub-models of Figs. 7 and 9 receive one user request, the retrieval time obtained from a sub-model shown in Fig. 9 is slightly higher than that of Fig. 6. This difference is due to the decision time taken by the main server of LMSi ( LMS to decide which disk server will retrieve the requested movie file. From Table-2, we also remark that the retrieval time of four, five, or six requests is greater than that of three requests. This difference is due to the waiting time spent in the buffer of the main server of LMSi ( LMS until one of the three disk servers DSx, DSy, and DSz ( DS become free. As a conclusion, the number of disk servers in each LMSi (LMS should be a large enough to handle a large number of user requests. Furthermore, such disk servers should work together in a parallel manner to handle the user requests. This conclusion is agreed with that obtained by a simulation method [6, 7, 10, 12, 32].

 Table 2.  The results of the ART performance measure (msec)

	Nmr
	Retrieval sub-model

(shown in Figure 6)

(sub-model-III in model A or B)
	Retrieval sub-model

(shown in Figure 8)

(sub-model-III in model-C)

	1
	315.675
	329.187

	2
	609.787
	341.551

	3
	903.037
	348.162

	4
	1189.111
	424.637

	5
	1468.551
	501.112

	6
	1757.775
	574.425


Table 3 illustrates the RRT and QoS performance results offered by the R-net MOD models for various workloads (multimedia requests). From these results, we can observe the following interesting points.


The request response time decreases as the number of disks used for retrieving the movie file is increased. The RRT performance results obtained from a model-C and a model-A (or a model-B) clarify this point. This result is due to a model-C performs its multimedia service processes in a parallel manner but a model-A (or a model-B) performs its multimedia service processes in a sequential manner.  This conclusion can be very useful in making decisions for investment in a new MOD system.

Table 3.  The results of the RRT and QoS performance measures


(Scan-EDF)

	QoS %

	1
	1.328
	75.25
	1.098
	91.07
	1.145
	29.112

	2
	2.422
	82.57
	2.121
	94.29
	1.188
	56.116

	3
	3.519
	85.24
	3.141
	95.51
	1.211
	82.576

	4
	4.621
	86.55
	4.135
	96.69
	1.477
	90.213

	5
	5.699
	87.71
	5.108
	97.88
	1.743
	95.611

	6
	6.722
	89.25
	6.114
	98.12
	1.998
	100.000


The type of disk scheduling algorithm that can be used in the MOD system effects on the RRT performance results. The RRT performance results obtained from model-A and model-B clarify this point. It is interesting to note that a model-A incorporates an EDF algorithm but a model-B incorporates a Scan-EDF algorithm. Therefore, the RRT performance results obtained from a model-A are better than those of a model-B. 


The request response time increases a very few msec when the number of users is increased. The RRT performance results obtained from a model-C clarify this point. Thus the delay a user experiences in viewing a movie is not affected too much by the number of users in the system.


The QoS of the MOD system increases as the number of multimedia requests increases. Furthermore, the QoS results provide insight on the max workload (multimedia requests) the MOD system is able to support. For example, the QoS of a model-C is 100% when the number of request is six. In other words, the max workload for a model-C is six requests. Thus, from the QoS performance results, we can decide the optimal number of multimedia requests that prevents the performance degradation of the MOD system.


Finally, we have compared the RRT results with those obtained by a simulation method [7, 12]. For example, when six users access the MOD system (model-C) at the same time, RRT = 1.998 sec. This result is close to that obtained by a simulation method, where RRT = 2.135 sec. This comparison gives us greater confidence that the performance results obtained from the developed R-net MOD models are realistic. Furthermore, the R-net MOD models have been developed in an accurate way.

7.  Conclusions

We have studied and analyzed the architecture of the MOD service system. To illustrate the dynamic behavior of the real MOD system, we have built three R-net performance models. The first model adopts the EDF disk scheduling algorithm. The second model adopts the Scan-EDF algorithm. These two models describe the dynamic behavior of one disk server when it performs the multimedia service processes. These models have been built in a simple way for explaining how the proposed R-net modeling technique can be used to model the dynamic behavior of real multimedia systems. In contrast, the third model describes the dynamic behavior of three disk servers when they work together in a parallel manner to perform the exact multimedia service processes. This realistic model can be extended to describe the real dynamic behavior of n disk servers.



In the developed R-net MOD models, we have concentrated our attention on studying and analyzing the following interesting multimedia problems:

· The storage problem has been studied through representing the mechanism of distributing the movie files across multiple disks to achieve data retrieval parallelism.

· The scheduling problem of the user requests has been studied through representing the EDF and Scan-EDF real-time disk scheduling algorithms. We have used this representation to analyze the effect of scheduling algorithms on the quality of service of the MOD system.

· The concurrent access problem has been studied through representing the mechanism of allowing multiple users to concurrently access the stored movie files.

· The data retrieval problem has been studied through representing the parallel mechanisms of retrieving the movie files from the desired disk array.

· The communication problem has been studied through representing the communication processes between the user and MOD service system.


To facilitate the analysis of the R-net models of the MOD service system, we have constructed them based on a modular technique. This modular technique provide an easy way to calculate the following performance measures: the quality of service, the request response time, the disk scheduling algorithm time, and the actual retrieval time.
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دراسة الأنظمة المتعددة الأوساط
سمير محمود كوريم

قسم نظم وهندسة الحاسب ، كلية الهندسة ، جامعة الأزهر

القاهرة،  مصر 
(قدّم للنشر في 3/12/2003م؛ وقبل للنشر في 11/12/2004م)

ملخص البحث. يتم خلال الأنظمة المتعددة الأوساط تناول بيانات تحتوي على نصوص وصور مرئية و صوتية، هذه البيانات هي التي تمثل المعلومات التي نشاهدها في الأفلام و البرامج التليفزيونية. هناك مشكلة يتم بحثها من قبل العلماء وهي عملية تزامن الصورة مع الصوت وكذا عملية تطوير ونمذجة وتحليل هذه الأنظمة المعقدة. ولذا في هذا البحث تم دراسة و تحليل نظام حقيقي للملتيمديا وذلك عن طريق عمل نموذج مبسط باستخدام تقنية تعرف بـ "ار- نت" . هذا النموذج سوف يساعد الباحثين على فهم كيفية عمل نموذج للأنظمة المتعددة الأوساط، ثم تم تنفيذ نموذج كامل حقيقي يمثل السلوك الديناميكي في الوقت الحقيقي لحدوث الاتصالات بين الكيانات المختلفة التي تمثل الأنظمة المتعددة الأوساط. وبعد دراسة وتحليل هذه النماذج تم عقد مقارنة لهذه النماذج ومن ثم تم استخلاص النتائج اللازمة لهذه الدراسة. ومن وجهة نظرنا يمكن أن تفيد هذه النتائج في معرفة كيفية نمذجة وتحليل الأنظمة المتعددة الأوساط. 
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